For 1990-2009 cars

#### Tools Required

J 23075 Third Clutch/Servo Piston Spring Compressor

1. Install J 23075 with the tool offset facing the rear of the transmission case.
2. Compress the servo piston assembly (106).
3. Remove the servo piston retainer ring (93).
4. Slowly release the pressure on the servo piston spring.
5. Remove J 23075 .
6. Remove the servo piston assembly (106).
7. Remove the return spring (103).
8. Remove the servo apply rod (102).
9. Inspect the servo apply rod for:

• | nicks

• | burrs

• | scoring