For 1990-2009 cars

## Timing Belt Cover Removal Front

1. Release the plastic retaining tabs on the wiring harness channel extension, from the right lower side of the wiring harness channel, and pull forward to remove.

Important: Use caution when releasing the retaining tabs to reduce the risk of breakage when removing the wiring harness channel cover.

2. Release the plastic retaining tabs on the wiring harness channel cover and remove the cover.
3. Remove the wiring from the wiring harness channel.

Note the wiring routing.

4. Remove the water pump pulley bolts.
5. Remove the water pump pulley.
6. Remove the power steering pump pulley bolts.
7. Remove the power steering pump pulley.
8. Remove the timing belt cover bolts.
9. Remove the timing belt cover.