For 1990-2009 cars

### Removal Procedure

1. Place the seat in the full forward and upright position.
2. Remove the left front seat track rear trim screw.
3. Remove the left front seat track front trim by unsnapping.
4. Remove the upper center pillar trim. Refer to Center Pillar Upper Trim Panel Replacement in Interior Trim.
5. Remove the carpet retainer. Refer to Carpet Retainer Replacement in Interior Trim.
6. Remove the left front lower seat belt bolt.
7. Remove the bolt from the left front seat belt retractor.
8. Remove the left front seat belt retractor upper bolt from the front seat shoulder belt guide adjuster.
9. Remove the screws (4) from the left front seat belt shoulder guide.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the left front seat belt shoulder guide.

Tighten
Tighten the left front seat belt shoulder guide screws (4) to 10 N·m (89 lb in).

2. Install the left front seat belt retractor upper bolt to the front seat shoulder belt guide adjuster.

Tighten
Tighten the left front seat shoulder belt to guide adjuster bolt to 35 N·m (26 lb ft).

3. Install the left front seat belt retractor.

Tighten
Tighten the left front seat belt retractor bolt to 35 N·m (26 lb ft).

4. Install the left front lower seat belt.

Tighten
Tighten the left front lower seat belt bolt to 35 N·m (26 lb ft).

5. Install the carpet retainer. Refer to Carpet Retainer Replacement in Interior Trim.
6. Install the upper center pillar trim. Refer to Center Pillar Upper Trim Panel Replacement in Interior Trim.
7. Install the front seat track front trim.
8. Install the front track rear trim screw.
9. Place the seat in the full forward and center position.