For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the exhaust resonator. Refer to Resonator Replacement .
3. Remove the exhaust muffler pipes from the resonator pipes.

### Installation Procedure

1. Install the exhaust muffler pipes to the resonator pipes and clamp in place.
2. Install the exhaust resonator. Refer to Resonator Replacement .
3. Check clearances and operate the exhaust system to check for leaks.
4. Lower the vehicle.