For 1990-2009 cars

### Removal Procedure

1. Remove front seat back headrest restraint. Refer to Front Seat Head Restraint Replacement .
2. Remove the front seat back panel. Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement .
3. Remove the headrest restraint release tab retainers from seat back using a flat-bladed tool. Discard release tab retainer.

### Installation Procedure

1. Install new headrest restraint release tab retainers to seat back.
2. Install the front seat back panel. Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement .
3. Install front seat back headrest restraint. Refer to Front Seat Head Restraint Replacement .