For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment floor carpet. Refer to Rear Floor Trim Plate Replacement .
2. Remove the two push retainers.
3. Remove the spare tire cover.
4. Remove the protect edge (2) around seat back opening.
5. Remove the push retainers (3).
6. Disconnect electrical connection and unroute wiring from the panel.
7. Remove the shock tower cover (1).
8. Remove the LH compartment side trim.

### Installation Procedure

1. Install the LH compartment side trim.
2. Install the shock tower cover (1).
3. Route the electrical wiring around the side trim and connection the electrical connection.
4. Install the push retainers (3).
5. Install the protect edge (2) around seat back opening.
6. Install the spare tire cover.
7. Install the two push retainers.
8. Install the rear compartment floor carpet. Refer to Rear Floor Trim Plate Replacement .