For 1990-2009 cars

## Speaker Grille Replacement Front Door

### Removal Procedure

1. Disable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Disabling the SIR System in SIR.
2. Remove the trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the speaker grille clips.
4. Remove the speaker grille.

### Installation Procedure

1. Install the speaker grille.
2. Install the speaker grille clips.
3. Install the trim panel. Refer to Front Side Door Trim Panel Replacement .
4. Enable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Enabling the SIR System in SIR.