For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rear fascia. Refer to Rear Bumper Fascia Replacement .
3. Remove the screws (2) from the rear fascia retainer (1).
4. Remove the retainer (1) from the rear quarter panel.

### Installation Procedure

1. Install the retainer (1) to the rear quarter panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws (2) to the rear fascia retainer.

Tighten
Tighten the rear fascia retainer screws to 10 N·m (89 lb in).

3. Install the rear fascia. Refer to Rear Bumper Fascia Replacement .
4. Lower the vehicle.