ERRATIC A/C COMP. OPERATION POSSIBLE POWER STEERING SW.. Cadillac Cimarron 1985

For 1990-2009 cars

# ERRATIC A/C COMP. OPERATION POSSIBLE POWER STEERING SW.

#### VEHICLES AFFECTED: ALL 1985-87 'J' MODELS

Some 1985-1987 Cimarrons may experience erratic A/C compressor operation. This condition may be caused by a corroded power steering pressure switch. To diagnose this condition, disconnect the power steering pressure switch and jumper across the connector terminals while the compressor is operating erratically. If the compressor stops cycling erratically, replace the power steering pressure switch, P/N 10041728. Should the compressor continue to cycle erratically, refer to the appropriate Section of the Service Manual for FURTHER DIAGNOSIS.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim .3 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.