REVISED FRONT WHEEL TOE SPECIFICATION MANUAL REVISION. Cadillac Cimarron 1985

For 1990-2009 cars

# REVISED FRONT WHEEL TOE SPECIFICATION MANUAL REVISION

#### MODELS AFFECTED: 1982-1985 CIMARRONS

The front wheel toe service specification for 1982 through 1985 Cimarrons has been revised. The specifications shown below should be used whenever adjusting front wheel alignment.

SERVICE TOE SPECIFICATION --- ------------- Per Wheel -.06 DEG +.10 DEG Sum -.12 DEG +.20 DEG

CAMBER +.85 DEG +.65 DEG

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.