NEW WEATHERSTRIP FOR VISTA VENT WATER LEAK REPAIR. Cadillac Cimarron 1984

For 1990-2009 cars

# NEW WEATHERSTRIP FOR VISTA VENT WATER LEAK REPAIR

#### MODELS AFFECTED: 1982, 1983 AND 1984 CIMARRON

Some 1982, 1983 and 1984 Cimarrons may experience water leaks at the vista vent. This condition may be caused by either inadequate weatherstrip sealing and/or vista vent glass panel hinge or latch assembly bushings that are split due to over tightening the attaching screws.

If the hinge or latch assembly bushing is split, replace with P/N 20586100 and torque the attaching screws to 3 N.m (26 inch pounds) (not 6 N.m, 53 inch pounds as previously specified). Refer to Item #2 and #16 in Figure 1.

For warranty replacement of bushing(s), use labor Operation T6106 at .2 hour (one or all). If the weatherstrip is leaking, replace with P/N 20534581 as follows:

1. Remove the vent assembly.

2. Break adhesive bond between weatherstrip and gutter around perimeter of opening and remove weatherstrip. Application of heat (as with a hot air gun or adhesive removing solvent) applied to weatherstrip gutter speeds weatherstrip removal.

3. Remove adhesive remaining in the weatherstrip gutter with an adhesive removing solvent.

4. Apply a coat of black adhesive to weatherstrip gutter (Figure 2). Be sure lap joints in gutter are covered with adhesive.

5. Apply a coat of adhesive to bonding surface of weatherstrip. When cement becomes tacky, insert weatherstrip into gutter for final bond. The joint of the weatherstrip must be located at center of sides.

6. Using a nozzle-type applicator, apply a bead of black weatherstrip adhesive between outer edge of weatherstrip and body opening.

For warranty purposes use labor Operation C1380 at .8 hour to replace the weatherstrip.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.