SERVICE MANUAL UPDATE-REVISED THROTTLE BODY FUEL RAIL TORQUE. Cadillac Cimarron 1988

For 1990-2009 cars

# SERVICE MANUAL UPDATE-REVISED THROTTLE BODY FUEL RAIL TORQUE

#### MODELS AFFECTED: 1987-1988 CIMARRONS

The throttle body attaching bolt torque and the fuel rail attaching bolt torque specifications are incorrect in some areas of the Service Manual. The correct torque specifications should be:

Throttle body to plenum attaching bolts -- 25 N-m (18 lbs. ft.)

Fuel rail to intake manifold attaching bolts -- 10 N-m (88 lbs. in.)

Intake plenum attaching bolts -- 21 N-m (16 lbs. ft.)

The above corrections should be made in the Service Manual at the following locations:

1987 Cimarron Service Manual

- Figure C2-8, page 6E3-C2-7 -- change Item 5 torque to read (88 lbs. in.).

- Page 6E3-C2-7, column 2, "Fuel Rail Installation" -- after installation step two, change to "Tighten attaching bolts to 10 N-m (88 lbs. in.)".

1988 Cimarron Service Manual

- Figure C2-11, page 6E3-C2-7 -- change Item 5 torque to read 10 N-m (88 lbs. in.).

- Page 6E3-C2-9, column 1, "Plenum Installation" -- after installation step 5, change to "Tighten throttle body bolts to 25 N-m (18 lbs. ft.)".

- Page 6E3-C2-10, top of column 1 -- change to "Tighten attaching bolts to 10 N-m (88 lbs. in.)".

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.