PAINT INFORMATION (ASSEMBLY PLANT USAGE). Cadillac Cimarron 1988

For 1990-2009 cars

# PAINT INFORMATION (ASSEMBLY PLANT USAGE)

The listings of 1988 paint codes contained in this bulletin will enable dealers to order the necessary paint materials required for effective field repairs.

The list of colors indicates the suppliers ordering codes for exterior, interior, vinyl roof moldings, and paint stripe colors.

Listed below is a current listing of the various Cadillac Assembly Plants and their suppliers. It should be noted, however, that paint suppliers are subject to change.

Assembly Plant Paint Type Paint Supplier Paint Codes -------------- ---------- -------------- ----------- *Fleetwood Dispersion Lacquer Inmont All

Hamtramck C/C Enamel DuPont All

Hamtramck (Allante) C/C Enamel PPG All

Orion C/C Enamel PPG All

Janesville Dispersion Lacquer DuPont All

*Arlington Dispersion Lacquer DuPont All

Other manufacturers produce service paint which could perform satisfactorily for field repairs. Paint suppliers in your area can provide you with information regarding these materials.

The paint listed in this bulletin is (or soon will be) available from local paint suppliers.

* Fleetwood stopped production of the Brougham on December 1987 and Arlington will start production of the Brougham on February 1988.

The Service Parts Identification (SPID) label illustrated in Figure 1 is located on the inside of the trunk panel or the spare tire cover. This label contains the paint codes needed to identify the paint materials for field repairs. Note that this label identifies the paint code along with the WA# for that paint code. It is equally important to use this WA# along with the paint code to identify the correct repair materials. This is especially true for codes #17 Pearl Gray and #50 Flax, where the WA# identifies the clearcoat repair material from the dispersion lacquer repair material. Care should be taken to transfer the SPID label or its information if the panel to which the label is affixed requires, replacement. Replacement SPID labels are not available.

1988 MODEL PAINT INFORMATION EXTERIOR -------- Paint Color PPG/ Code Name WA# Dupont Ditzler

08 M. K. Pink 7795 2304 70748 11 White 3967 5338 2058

12 Silver Met. 8535 B8501 3746 13S Silver Met. C/C 9021 D8590 3822 14 Black Met. C/C 8767 B8701 3961 15 Med. Gray Met. 8573 B8502 3749 17 Pearl Gray 9057 B8702 3963 17 Pearl Gray C/C 9349 B8891 4083 22 Lt. Sapphire Blue Met.C/C 8966 B8703 3964 26 Lt. Sapphire Blue Met. 8964 B8704 3966 28 Black Sapphire Met. C/C 8743 B8618 3885 29 Dk. Sapphire Blue Met. 8970 B8706 3968 30 Silver Met. C/C 9065 D8720 4010 32 Black Sapphire F/M 9058 B8892 4087 40 White C/C 8554 B8469 3680 41 Black C/C 8555 99S 9700 43 Burgundy Met. C/C 9589 D8892 4127 46 Gold Met. C/C 9071 D8723 4011 47 Red C/C 9547 D8891 4126 48 Black C/C 9588 99S 9729 50 Flax C/C 8557 B8475 3668 50 Flax 7694 B8318 3529 52 Cooper Beige 9179 B8870 4088 55 White Met. Tri-Coat 9069 D8722 4013B/C 4014TMid/C 57 Lt. Beechwood Met. 9180 B8872 4090 62 Lt. Beechwood Met. C/C 9089 B8877 4094 67 Dk. Antelope Met. C/C 9094 B8879 4096 69 Med. Beechwood Met. C/C 9091 B8880 4109 72 Med. Garnet Red Met. C/C 8979 B8713 3986 76 Dk. Garnet Red Met. C/C 8984 B8716 3989 80 Lt. Rosewood Met. C/C 8992 B8718 3993 82 Med. Rosewood Met. C/C 8990 B8719 3994 83 Med Sapphire Blue F/M/C/C 8993 B8720 3995 86 Antelope Beige C/C 9200 B8886 4101 87 Gunmetal Gray C/C 9243 B8729 4009 88 Dk. Gray Met. 8600 B8517 3788 89 Autumn Maple F/M 8237 B&385 3532 92 Gray Met. C/C 9532 D8886 4122 93 White Diamond 8933 B8609 3903 95 Lt. Antelope F/M C/C 9093 88889 4104

Paint Color Martin- Sherwin-Williams R-M Code Name WA# Senour ACME/Rogers Inmont ---- ---- --- ------ ----------- ------ 08 M. K. Pink 7795 32-8547 34442 12899 White 3967 30-3929 LIOA-2864 3-644 2080 12 Silver Met. 8535 30-5371 34380 15001 13S Silver Met. C/C 9021 30-5491 35369 15365 14 Black Met. C/C 8767 35877 35877 17002 15 Med. Gray Met. 8573 30-5372 34381 15004 17 Pearl Gray 9057 35878 35878 17001 17 Pearl Gray C/C 9349 37079 37079 18030 22 Lt. Sapphire Blue Met.C/C 8966 35879 35879 17003 26 Lt. Sapphire Blue Met. 8964 35865 35865 17005 28 Black Sapphire Met. C/C 8743 30-5520 35313 16003 29 Dk. Sapphire Blue Met. 8970 35866 35866 17007 30 Silver Met. C/C 9065 37008 37008 17485 32 Black Sapphire F/M 9058 37081 37081 18002 40 White C/C 8554 30-5295 33755 13570 41 Black C/C 8555 30-5296 33756 13572 43 Burgundy Met. C/C 9589 38792 38792 18626 46 Gold Met. C/C 9071 37009 37009 17486 47 Red C/C 9547 38860 38860 18627 48 Black C/C 9588 39126 39126 18628 50 Flax C/C 8557 30-5338 33942 18000 50 Flax 7694 30-5181 32703 13116 52 Cooper Beige 9179 37082 37082 18007 55 White Met. Tri-Coat 9069 37011-B/C 37011-B/C 38990 Mid/C 38990 Mid/C 17487 57 Lt. Beechwood Met. 9180 37084 37084 18008 62 Lt. Beechwood Met. C/C 9089 37088 37088 18003 67 Dk. Antelope Met. C/C 9094 37090 37090 18006 69 Med. Beechwood Met. C/C 9091 37091 37091 18004 72 Med. Garnet Red Met. C/C 8979 35894 35894 17021 76 Dk. Garnet Red Met. C/C 8984 35895 35895 17023 80 Lt. Rosewood Met. C/C 8992 35898 35898 17027 82 Med. Rosewood Met. C/C 8990 35896 35896 17026 83 Med Sapphire Blue F/M/C/C 8993 35900 35900 17028 86 Antelope Beige C/C 9200 37097 37097 18015 87 Gunmetal Gray C/C 9243 36724 36724 17038 88 Dk. Gray Met. 8600 30-5398 34407 15042 89 Autumn Maple F/M 8237 30-5244 33074 13131 92 Gray Met. C/C 9532 38861 38861 18629 93 White Diamond 8933 B/C-39244 B/C-39244 18632 M/C-39245 M/C-39245 95 Lt. Antelope F/M C/C 9093 37099 37099 18005

#### NOTE: C/C = Basecoat/Clearcoat F/M = Firemist B/C = Basecoat M/C = Mid-Coat

1998 MODEL PAINT INFORMATION INTERIOR --------

Paint Color Code Name WA# Dupont PPG/Ditzler Martin-Senour ---- ---- --- ------ ----------- ------------- 11N White 3835 8622-5 DEG. L/G -- 17172-5 DEG. 8536-12 DEG. S/C 90232 17029-12 DEG. UCV -183 12DN Graphite 7701 8345V L/G 33870 16963-5 DEG. S/G 33622 16905-12 DEG. UCV 2-1020 19N Black 848 428-5 DEG. L/G 9433 16615-5 DEG. 8535-12 DEG. S/G 9640 16918-12 DEG. UCV -120 2OBN Med. Sapphire 8842 C8813V L/G * S/G 16235 36470-12 DEG. UCV 2-1219 2ODN Very Dk Sapphire 8841 -- L/G -- 36571-5 DEG. C8770-12 DEG. S/G 16202 36479-12 DEG. UCV 2-1215 50AN Lt. Yellow 7042 C8388-5 DEG. L/G -- 16992-5 DEG. C8365-12 DEG. S/G 82674 17030-12 DEG. UCV 2-580 5OCN Very Dk. Yellow 8804 C8664-305-5 DEG. L/G -- 17141-5 DEG. C8664-306-12 DEG. S/G 82631 17152-12 DEG.

UCV 2-1168 6ICN Dk. Sienna 8856 C8811-5 DEG. L/G 26248 38220-5 DEG. S/G 25916 38382-12 DEG. UCV 2-1220 6IDN Very Dk. Sienna 9105 C8814-5 DEG. L/G 26253 38221-5 DEG. S/G 26254 38383-12 DEG. UCV 2-1293 65BN Med. Antelope 9102 C8806-5 DEG. L/G 26251 38602-5 DEG. S/G 26252 38219-12 DEG. UCV 2-1210 65CN Dk. Antelope 9245 C8809-5 DEG. L/G 26255 38222-5 DEG. S/G 26256 38384-12 DEG. UCV 2-1294 66BN Med. Beechwood 9098 C8805-5 DEG. L/G 26249 38601-5 DEG. S/G 26250 38218-12 DEG. UCV 2-1289 72CN Carmine 8577 C8563-5 DEG. L/G 72947 17076-5 DEG. C8540-12 DEG. S/G 72776 17085-12 DEG. UCV 2-1282 75CN Dk. Rosewood 8843 -- L/G 36572-5 DEG. C8774-12 DEG. S/G 72847 36474-12 DEG. UCV 2-1216 75DN Very Dk Rosewood 8844 C8812V L/G 51290 36504-5 DEG. S/G 51246 38381-12 DEG. UCV 2-1221 78CN Garnet Red 8781 C8624-5 DEG. L/G 17134-5 DEG. C8616-12 DEG. S/G 72799 17147-12 DEG. UCV 2-1173 78DN Very Dk 8827 D8748-5 DEG. L/G 51288 36500-5 DEG. Garnet Red D8747-12 DEG. S/G 51247 36473-12 DEG. UCV 2-1222 79CN Dk. Claret 4887 C8560-5 DEG. L/G 51085 16751-5 DEG. C8537-12 DEG. S/G 51170 17084-12 DEG. UCV 2-479 82CN Med. Dark Gray 8247 C8556-5 DEG. L/G 33873 16965-5 DEG. C8447-12 DEG. S/G 33665 16949-12 DEG. UCV 2-1048 82DN Dark Gray 8595 C8597-5 DEG. L/G 33874 17080-5 DEG. C8550-12 DEG. S/G 33824 17071-12 DEG.

Paint Color Sherwin-Williams R-M Code Name WA# ACME/Rogers Inmont ---- ---- --- ----------- ------ 11N White 3835 35574-5 DEG. 11526-5 DEG. 33777-12 DEG. 4402-12 DEG.

12DN Graphite 7701 33767-5 DEG. 16042-5 DEG. 32989-12 DEG. 13199-12 DEG.

19N Black 848 J4-8677-5 DEG. 12812-5 DEG. 92387 4401-12 DEG. 33024-12 DEG. 2OBN Med. Sapphire 8842 * 18060-5 DEG. 36470-12 DEG. 17096-12 DEG.

2ODN Very Dk Sapphire 8841 36571-5 DEG. 17095-5 DEG. 36479-12 DEG. 17094-12 DEG.

50AN Lt. Yellow 7042 32351-5 DEG. 11528-5 DEG. 33778-12 DEG. 9558-12 DEG.

5OCN Very Dk. Yellow 8804 35440-5 DEG. 16050-5 DEG. 35473-12 DEG. 18630-12 DEG.

6ICN Dk. Sienna 8856 38220-5 DEG. 18045-5 DEG. 38382-12 DEG. 17104-12 DEG.

6IDN Very Dk. Sienna 9105 38221-5 DEG. 18050-5 DEG. 38383-12 DEG. 18051-12 DEG.

65BN Med. Antelope 9102 38602-5 DEG. 16069-5 DEG. 38219-12 DEG. 16063-12 DEG.

65CN Dk. Antelope 9245 38222-5 DEG. 18052-5 DEG. 38384-12 DEG. 18053-12 DEG.

66BN Med. Beechwood 9098 38601-5 DEG. 18046-5 DEG. 38218-12 DEG. 18047-12 DEG.

72CN Carmine 8577 34607-5 DEG. 16046-5DEG. 34639-12 DEG. 15084-12 DEG.

75CN Dk. Rosewood 8843 36572-5 DEG. 17098-5 DEG. 36474-12 DEG. 17097-12 DEG.

75DN Very Dk Rosewood 8844 36504-5 DEG. 17099-5 DEG. 38381-12 DEG. 18631-12 DEG.

78CN Garnet Red 8781 35433-5 DEG. 17085-5 DEG. 35468-12 DEG. 16055-12 DEG.

78DN Very Dk 8827 36500-5 DEG. 17089-5 DEG. Garnet Red 36473-12 DEG. 17090-12 DEG.

79CN Dk. Claret 4887 30814-5 DEG. 17090-12 DEG. 34638-12 DEG. 8763-12 DEG.

82CN Med. Dark Gray 8247 33769-5 DEG. 14088-5 DEG. 33714-12 DEG. 14009-12 DEG.

82DN Dark Gray 8595 34611-5 DEG. 15095-5 DEG. 346012-12 DEG. 15268-12 DEG.

#### NOTE: Painted parts on the Instrument Panel have a 5 DEG. gloss finish and the steering column parts have a 12 DEG. gloss finish.

* Not Available

#### 1988 CADILLAC PAINT STRIPE COLORS

Paint Color Code Name WA# Dupont PPG/Ditzler Martin-Senour ---- ---- --- ------ ----------- ------------- 11A White 3967 5338 2058 32-3929

14A Lt.Gray 8670 C8529 33856 32-26729 18A Gun Metal 8291 C8441 33750 32-26700 19A Black 848 99 9000/9300 3069

20A Lt. Sapphire 9193 C8786 16319 36466 21A Dk. Sapphire 9103 C8787 16313 36464 34A Med. Beechwood 9274 D8869 26298 38403 49A Antelope Beige 9200 B8886 4101 38402 55A Gold 8589 D8276 25509 32-28703 59A Copper Beige 8973 D8753 25894 36462 66A Orange 8002 45261 60909 32-26337

67A Dk. Brown 8001 45260 25088 32-26336

68A Lt. Rosewood 8874 C8782 51283 36460 72A Dk. Rosewood 8872 C8783 51282 36459 73A Dk. Garnet 9106 C8790 51286 36465 75A Red 4721 43592 72128 32-26272

76A Garnet Red 8852 C8643 51211 32-26780 79A Dk. Claret 8663 C8525 51167 32-26728

Paint Color Sherwin-Williams R-M Code Name WA# ACME/Rogers Inmont ---- ---- --- ----------- ------ 11A White 3967 L10A-2864 5644 2080 14A Lt.Gray 8670 34869 15165 18A Gun Metal 8291 34102 14036 19A Black 848 L10B-1738 3000/4590 A946 20A Lt. Sapphire 9193 36466 17057 21A Dk. Sapphire 9103 36464 17055 34A Med. Beechwood 9274 38403 17537 49A Antelope Beige 9200 38402 17538 55A Gold 8589 34105 15076 59A Copper Beige 8973 36462 17053 66A Orange 8002 J4-8728 25455 9500 67A Dk. Brown 8001 J4-8727 25460 9502 68A Lt. Rosewood 8874 36460 17051 72A Dk. Rosewood 8872 36459 17050 73A Dk. Garnet 9106 36465 17056 75A Red 4721 J4-7191 11892 4518 76A Garnet Red 8852 35566 16086 79A Dk. Claret 8663 34868 15071

#### 1988 CADILLAC VINYL ROOF MOLDING COLORS

Paint Color Sherwin-Williams Code Name WA# Dupont PPG/Ditzler Martin-Senour ---- ---- --- ------ ----------- ------------- 11T White 8936 * 2-130 32-26851 13T Silver Met. 7781 B8402 2-1052 32-26704 17T Pearl Gray 9057 B8702 2-1265 36604 18T Black Met. 8767 B8701 2-1269 36594 19T Black 848 99 -120 32-16082

22T Lt. Sapphire Blue Met. 8966 B8703 2-1271 36595 26T Lt. Sapphire Blue Met. 8964 B8704 2-1313 37031 28T Black Sapphire Met. 8743 B8628 2-1273 36593 29T Dk. Sapphire Blue Met. 8970 B8706 2-1295 37032 37T Flax 7694 D8377 2-957 32-26643 62T Lt. Beechwood Met. 9089 B8877 2-1314 38561 67T Dk. Antelope Met. 9094 B8879 2-1298 38564 69T Med. Beechwood Met. 9091 B8880 2-1299 38562 72T Med. Garnet Red Met. 9979 B8713 2-1268 36596 76T Dk. Garnet Red 8984 B8716 2-1272 36597 82T Med. Rosewood Met. 8990 B8719 2-1266 36598 83T Med. Sapphire Blue Met. 8993 B8720 2-1274 36600 84T Gun Metal Met. 7782 B8403 2-1053 32-26705 85T Lt. Rosewood Met. 8992 B8718 2-1285 36599 86T Lt. Antelope 9200 B8886 2-1300 38567 95T Lt. Antelope Met. 9093 B8889 2-1301 38563

Paint Color R-M Code Name WA# ACME/Rogers Inmont ---- ---- --- ----------- ------ 11T White 8936 35781 16110 13T Silver Met. 7781 34123 14039 17T Pearl Gray 9057 36604 17067 18T Black Met. 8767 36594 17065 19T Black 848 J4-1990/ 9739 4416 22T Lt. Sapphire Blue Met. 8966 36595 17066 26T Lt. Sapphire Blue Met. 8964 37031 18071 28T Black Sapphire Met. 8743 36593 17068 29T Dk. Sapphire Blue Met. 8970 37032 17079 37T Flax 7694 33180 13162 62T Lt. Beechwood Met. 9089 38561 18074 67T Dk. Antelope Met. 9094 38564 18075 69T Med. Beechwood Met. 9091 38562 18076 72T Med. Garnet Red Met. 9979 36596 17072 76T Dk. Garnet Red 8984 36597 17073 82T Med. Rosewood Met. 8990 36598 17075 83T Med. Sapphire Blue Met. 8993 36600 17074 84T Gun Metal Met. 7782 34124 14040 85T Lt. Rosewood Met. 8992 36599 17077 86T Lt. Antelope 9200 38567 18078 95T Lt. Antelope Met. 9093 38563 18079

* Not Available

#### 1988 CIMARRON STRIPE COMBINATIONS

Paint Code WA# CODES UPPER/LOWER COLOR COMBINATIONS ---- --------- ------------------------------ O1A 3967/4721 White (11A) Red (75A) 02A 3967/8670 White (11A) Lt. Gray (14A) 03A 3967/7456 White (11A) Lt. Sapphire (20A) 09A 3967/9103 White (11A) Dk. Sapphire (21A) 33A 7456/9103 Lt. Sapphire (20A) Dk. Sapphire (21A) 43A 8973/3967 Copper Beige (59A) White (11A) 45A 8973/8002 Copper Beige (59A) Dk. Brown (67A) 80A 4721/9103 Red (75A) Dk. Sapphire (21A) 85A 4721/8670 Red (75A) Lt. Gray (14A) 89A 4721/8291 Red (75A) Dk. Gray (18A) 93A 4721/848 Red (75A) Black (19A) 94A 8001/8002 Dk. Brown (67A) Orange (66A)

EXTERIOR PLASTIC PARTS

All 1987 Cadillacs have exterior parts made of various types of plastic materials that require specific procedures to obtain high quality refinishing results. Included in this bulletin is a chart listing the different types of plastic materials used on 1987 models. For best results when painting is required, determine the type of plastic material from the chart. Then follow the correct paint procedure, depending upon what painting material and equipment is available.

PLASTIC TYPE SYMBOL

Thermoset Urethane RRIM Thermoplastic Urethane TPU Thermosetting Polyester UP (SMC) Thermoplastic Urethane RIM Thermoplastic Elastomer TPE Xenoy --

A. GENERAL PAINT PROCEDURE FOR EXTERIOR FLEXIBLE PLASTICS

Polyvinylchloride (PVC), Polyurethane (PUR, TPUR, RRIM, RIM), Thermoplastic Elastomer (TPE), Thermoplastic Polyester (SMC), EPDM Rubber (Supplied in Prime).

There are a multitude of finishing systems available on the market for painting and/or repairing flexible plastic parts. Following is a general outline of painting procedures, including a list of available products. Refer to the manufacturer's literature available through your jobber for details on proper mixing and application.

1. Thoroughly clean part by washing with a suitable cleaning solvent* to remove all surface contaminates.

#### NOTICE: Previously painted parts that show signs of cracking, peeling or improper adhesion must be stripped before repainting. The old finish may be removed with any commercially available chlorinated solvent stripper or lacquer thinner.

#### NOTICE: Do not soak parts longer than necessary to remove the old paint to avoid swelling.

2. Scuff sand to an even dull appearance the entire surface to be painted with fine (400 grit) sandpaper and feather edge any damaged areas and rewash as in Step A.

#### NOTICE: Unpainted parts do not require sanding prior to painting, but should be thoroughly cleaned as in Step A.

3. Apply two (2) thin coats of primer when required per top coat manufacturer's recommendation and allow to completely dry before proceeding. (For most products, approximately 30 minutes).

4. Prepare color coat according to the manufacturer's recommendation and apply sufficient double coats to develop the proper shade. For best results, allow a few minutes flash time between each double coat and allow to completely dry before using.

5. Following is a list of some of the products available for painting flexible plastic.

PPG/Ditzler Elastomeric Primer - DPX844 PPG/Ditzier Flexative - DX369 (Permanent Flexible Urethane Additive) PPG/Ditzler Flex Additive - DX1798 (Non-Urethane Additive) DuPont (Flexlar-350S (Flexible Additive) Sherwin-Williams Multi-Flex - V6V299 Acme/Rogers Multi-Flex - 68/4068 Martin-Senour Flex Additive - 3084

*Cleaning Solvents

a. DuPont Prep-Sol b. Rinshed-Mason Pre-Kleano 900 c. PPG/Ditzler Acryli-Clean DX330 d. Sherwin-Williams R7K 156 e. Acme 88; Rogers 088 f. Martin-Senour 6383

B. NYLON - Will be supplied in prime. Use the same procedure to refinish as on sheet metal parts.

C. ACRYLONNITRILE-BUTADIENE-STYRENE (ABS) - No prime required; paint with acrylic lacquer.

D. POLYESTER PARTS (UP, PBTP) - Wilibe supplied in prime and/or black paint. Use the same procedure to refinish or repair as on sheet metal parts.

E. POLYPROPYLENE - Interior parts.

1. Wash surface thoroughly with enamel reducer. (Do not use wax and grease removers.)

2. Apply primer immediately and allow to dry completely before color coating.

3. Color coat with lacquer or enamel reduced and applied according to the manufacturer's recommendation.

4. Materials:

Cleaning Solvent - DuPont 3812S Enamel Reducer PPG/Ditzler DTE-101 or DTE-102 "Bobcat" Enamel Reducer Primer - DuPont 3293 GM 1052364 PPG/Ditzler DPX-800 Sherwin-Williams P3C24* ACME/Rogers 524/4524* Martin-Senour 6242*

* Good on Polyethylene and Polypropylene Parts

F. Xenoy - will be supplied in colors. Use the same procedure to refinish or repair as on sheet metal parts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.