PAINT INFORMATION ALL 1982 MODELS. Cadillac Cimarron 1982

For 1990-2009 cars

# PAINT INFORMATION ALL 1982 MODELS

ATTACHED ARE 1982 CHARTS TO FACILITATE QUICK IDENTIFICATION OF PAINT NEEDED FOR DIFFERENT APPLICATIONS.

THESE CHARTS COVER EXPERIOR COLOURS AND INTERIOR COLOURS PAINT STRIPE COLOURS AND MISCELLANEOUS PAINT ITEMS WITH INDICATION OF GM PAINT CODES, COLOUR NAME AND STOCK NUMBERS BY PAINT SUPPLIERS CPI (DITZLER), (R-M), DUPONT, CIL AND FISHER.

ADDITIONAL PAINT STRIPE COLOURS AND MISCELLANEOUS PAINT ITEMS WILL BE PRINTED AT A LATER DATE.

#### NOTE:

ALL VEHICLES BUILT AT FREMONT, CALIFORNIA AND NORWOOD, OHIO WILL BE PAINT WITH HIGH-SOLIDS ENAMEL TOP COATS. THE HIGH-SOLIDS ENAMELS LISTED BELOW WILL REQUIRE A SPECIAL FORMULA AND CANNOT BE REPAIRED WITH THE STANDARD COLOURS EVEN THOUGH THEY ARE IDENTIFIED WITH THE STANDARD GM COLOUR CODE. CHECK THE VEHICLE BODY PLATE FOR PAINT TYPE.

VEHICLES WITH AN 'E' ARE HIGH-SOLIDS ENAMEL. VEHICLES WITH AN 'L' ARE LAC- QUER AND 'W' IDENTIFIES WATER BASE AND CAN USE THE STANDARD REFINISH COLOURS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.