SERVICE MANUAL UPDATES PISTON TO BORE CLEARANCES. Cadillac Cimarron 1984

For 1990-2009 cars

# SERVICE MANUAL UPDATES PISTON TO BORE CLEARANCES

#### MODELS AFFECTED: 1982-1986 CIMARRONS

The 1982-1986 Cimarron Service Information Manual specifications for the piston-to-bore and piston-to-pin clearances for 2.OL L-4 engines need to be corrected:

Piston-to-bore clearance: = .0007" - .0017" (.017mm - .043mm)

Piston-to-pin clearance: 1982-1984 = .00026" - .00037" (.007mm - .009mm)

1985-1986 = .0002" - .0007" (Production) (.005mm - .018mm)

1985-1986 = .0004" - .0009" (Revised Service Parts) (.010mm - .022mm)

Please make the appropriate changes to your Service Information Manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.