STEERING COLUMN REPLACEMENT INCORRECT PART INFORMATION. Cadillac Cimarron 1988

For 1990-2009 cars

# STEERING COLUMN REPLACEMENT INCORRECT PART INFORMATION

#### MODELS AFFECTED: 1987-1988 CIMARRONS

This bulletin supersedes Bulletin T-88-44, Group 3B, which should be destroyed.

If diagnosis of a steering column condition leads to replacement of the column, the following part numbers must be used:

1987 1988 Application ---- ---- ----------- 7844369 26006871 Cimarron with manual transaxle 7844367 26006872 Cimarron with automatic transaxle

For warranty purposes use Labor Operation E7660 at .8 hour and an add time of .4 hour to color coat with material allowance GB.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.