ROCKER COVER OIL LEAK NEW ROCKER COVER GASKET. Cadillac Cimarron 1985

For 1990-2009 cars

# ROCKER COVER OIL LEAK NEW ROCKER COVER GASKET

#### MODELS AFFECTED: 1985-1986 CIMARRON EQUIPPED WITH 2.8L - V-6 ENGENES

Some 1985 Cimarrons equipped with the 2.8L V-6 engine may exhibit oil leaks from the rocker arm cover area.

To correct this condition, the 1986 rocker arm cover gasket (P/N 14089253) can be installed. This gasket does not supersede the use of RTV, but is available as an optional method for sealing the rocker arm cover.

For warranty purposes, please use the following labor operations and times.

Labor Operation Time --------------- ---- 90300 (Right Bank) 1.2 hours J0301 (Left Bank) .8 hours J0307 (Both Banks) 1.8 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.