GARNISH MOLDING RATTLE INSTALL NEW RETAINER CLIPS. Cadillac Cimarron 1987

For 1990-2009 cars

# GARNISH MOLDING RATTLE INSTALL NEW RETAINER CLIPS

#### MODELS AFFECTED: 1985-1988 CIMARRONS

Some 1985-1988 Cimarrons may experience a garnish molding rattle. This may be caused by body build variations in the upper rail of the door openings.

This condition may be repaired by installing molding retainer clips, P/N 20286225, as shown in the illustration. Use two clips per molding.

For warranty purposes use Labor Operation C3028 (RH) at .2 hour or C3038 (LH) at .2 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.