TAIL LAMP ASSEMBLY REMOVAL PROCEDURE. Cadillac Cimarron 1986

For 1990-2009 cars

# TAIL LAMP ASSEMBLY REMOVAL PROCEDURE

#### VEHICLES AFFECTED: 1986 Cadillac Cimarron

The following service procedure should be used when removing 1986 6JG69 style tail lamp assemblies.

#### Removal

1. Remove screws securing license plate to license plate pocket.

2. Remove screws, item 2, Figure No. 1.

3. Open rear compartment lid and remove four (4) nuts, Item 3, Figure No. 1.

4. Remove lamp assemblies item 1. Figure No. 1.

5. To install, reverse removal procedure.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.