LOOSE INSTRUMENT PANEL TRIM PLATE. Cadillac Cimarron 1982

For 1990-2009 cars

# LOOSE INSTRUMENT PANEL TRIM PLATE

RIGHT HAND INSTRUMENT PANEL ACCESSORY TRIM PLATE REPLACEMENT

Some 1982 Cimarrons may exhibit a condition where the trim plate surrounding the cigar lighter, defogger switch and AC/heater controls is loose or allows light from around the AC/heater controls.

To correct cars exhibiting this condition, replace the trim plate with new trim plate, P/N 1623880, by performing the following procedure:

1. Remove trim plate from instrument panel.

2. Disconnect wiring to cigar lighter and defogger switch.

3. Remove cigar lighter and defogger switch from trim plate.

4. Remove spring clips from trim plate and discard trim plate.

5. Install defogger switch, cigar lighter and spring clips on new trim plate, P/N 1623880.

6. Install "U" nut, P/N 11504531, in instrument panel as shown in illustration.

7. Connect wiring to defogger switch and cigar lighter.

8. Install trim plate on instrument panel.

9. Install retaining screw as shown in the illustration.

For warranty purposes, use Operation No. C2340, Trim Plate - Replace, at 0.2 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.