COIL WIRE SERVICE IDENTIFICATION OF PROPER COIL. Cadillac Cimarron 1986

For 1990-2009 cars

# COIL WIRE SERVICE IDENTIFICATION OF PROPER COIL

#### VEHICLES AFFECTED: 1982-86 'J' Models Equipped With 1.8L (VIN CODE G) and 2.0L (VIN Code P)

When replacing the coil wire on the 1982-86 'J' model with the 1.8L carbureted engine or the 2.0L fuel injected engines the proper part number wire must be used to insure proper engagement of the terminal and sealing against contamination. (See Illustration attached).

Part Number Model Year ----------- ---------- 12036900 1982 - 84 12036972 1985 - 86

#### NOTICE: If the 1982-84 part is used on the 1985-86 models, the boot will be too long on the distributor end and may not allow proper terminal engagenent. Also, the boot will be too short on the coil end and a poor seal against contamination may result.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.