DEFROSTER ARM LINK UNHOOKED OR BROKEN (NEW DESIGN PARTS). Cadillac Commercial Limo/Hearse Chassis 1991

For 1990-2009 cars

# DEFROSTER ARM LINK UNHOOKED OR BROKEN (NEW DESIGN PARTS)

#### SUBJECT: DEFROSTER ARM LINK UNHOOKED OR BROKEN (NEW PARTS)

#### VEHICLES AFFECTED: 1991 "C" MODELS

#### CONDITION:

---------- Some 1991 Cadillac DeVilles and Fleetwoods may experience no A/C - Defrost mode door operation causing no mode change from defrost or A/C.

#### CORRECTION:

----------- The above condition may be corrected by performing one of the following procedures:

1. Verify that the defrost actuator arm/link to the A/C defrost mode door has not slipped off the hook at the end of the crank. The link can be held in place by a push-on nut, part number #11501927.

2. Verify that the defrost actuator bracket has not broken away from the modular duct. This would require replacement of the modular duct, part number #52453656.

3. Inspect the hook on the A/C defrost door crank and the hook itself to ensure it has not broken. This would require replacement of the defroster door, part number #52453658.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.