POOR FIT OF LITTER CONTAINER REPAIR PROCEDURE. Cadillac Commercial Limo/Hearse Chassis 1991

For 1990-2009 cars

# POOR FIT OF LITTER CONTAINER REPAIR PROCEDURE

#### SUBJECT: LITTER CONTAINER WILL NOT SLIDE ONTO BRACKET (REMOVE 20MM OF PROGRAMMER FROM FRONT TAB)

#### VEHICLES AFFECTED: 1991 'C'

Some 1991 DeVilles and Fleetwoods may experience a condition where the litter container will not slide easily onto its bracket. This condition is caused by an interference between the A/C programmer and the hush panel. To repair this condition, use the following procedure:

1. Remove hush panel screws.

2. Remove glove box module and set aside.

3. Disconnect air mix valve link rod from programmer.

4. Remove vacuum and electrical connectors.

5. Remove programmer screws.

6. Remove programmer through glove box opening.

7. Place programmer on a table and remove 20mm (3/4") from the front tab. Refer to Figure 2.

8. Reassemble programmer and hush panel.

Use the most applicable Labour Operation and Time from the Canadian Labour Time guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.