STRIPPED OIL PAN DRAIN PLUG (INSTALL NEW DRAIN PLUG). Cadillac Commercial Limo/Hearse Chassis 1991

For 1990-2009 cars

# STRIPPED OIL PAN DRAIN PLUG (INSTALL NEW DRAIN PLUG)

REVISION 03/11/93

THIS BULLETIN IS BEING REVISED TO CORRECT TAP SIZE. THE REVISED INFORMATION WILL APPEAR ON AN UPDATE BULLETIN. THE REMAINDER OF THIS BULLETIN WILL NOT BE PUBLISHED. WARRANTY ADMINISTRATION HAS BEEN NOTIFIED OF ALL CHANGES AND THE WARRANTY CLAIMS PROCESSING SYSTEM HAS BEEN UPDATED.

SOME 1991 DEVILLES, ELDORADOS, AND SEVILLES MAY EXPERIENCE STRIPPING OF THE ENGINE OIL PAN DRAIN PLUG THREADS DURING ROUTINE SERVICE. THIS CONDITION MAY BE CAUSED BY WELD SPATTER ON THE THREADS OF THE OIL PAN DRAIN HOLE FROM THE MANUFACTURING OPERATION.

TO REPAIR THIS CONDITION INSTALL A NEW DRAIN PLUG, P/N 10017615, AND RETAP THE OIL PAN THREADS WITH AN M12 X 1.75 TAP.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

FOR WARRANTY PURPOSES USE LABOR OPERATION T6556 AT .4 HOUR.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 CADILLAC MOTOR CAR DIVISION, GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.