INFO. ON SERVICE PARTS FOR COMPUTER COMMAND RIDE (CCR). Cadillac Commercial Limo/Hearse Chassis 1993

For 1990-2009 cars

# INFO. ON SERVICE PARTS FOR COMPUTER COMMAND RIDE (CCR)

#### SUBJECT: INFORMATION ON SERVICE PARTS FOR COMPUTER COMMAND RIDE (CCR) FRONT STRUT

#### MODELS: 1993 CADILLAC DEVILLE (WITH FW1 SUSPENSION) VIN BREAKPOINTS: P4329854 TO E.O.P.

APPROXIMATELY 4,000 1993 VEHICLES EQUIPPED WITH COMPUTER COMMAND RIDE (CCR) WERE BUILT WITH THE 1994 CCR STRUT ASSEMBLY. VEHICLES BUILT WITH FRONT STRUT, P/N 22139715, AND BROADCAST CODE 3E SHOULD BE SERVICED USING THE FOLLOWING 1993 COMPONENTS:

REMOVE ADD OR REPLACE WITH ====== ===================

STRUT, FRONT SUSPENSION 22139715 22064321 SEAT, FRONT SPRING 22119701 22128884 SPACER, FRONT SPRING 22098980 BUMPER, JOUNCE RING 22105516 SHIELD, FRONT SUSPENSION STRUT 22128834 22136273 SPRING, FRONT 22076736-38 22078111 22076739-41 22078113 22076880 22078113

PARTS ARE EXPECTED TO BE AVAILABLE ON DECEMBER 13, 1993.

IF ANY OF THE ABOVE COMPONENTS ON THE LEFT OR RIGHT STRUT ASSSEMBLY NEEDS REPLACEMENT, THE REPLACEMENT MUST BE DONE IN PAIRS ON BOTH THE LEFT AND RIGHT SIDE. ADDITIONALLY, WHEN ONE COMPONENT REQUIRES REPLACEMENT, ALL OF THE ABOVE COMPONENTS MUST BE REPLACED. REFER TO SECTION 3C IN THE SERVICE MANUAL.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.