Accessory Removal. Cadillac Concours 1996

For 1990-2009 cars

### Drive Belt Idler Pulley Removal Procedure

1. Loosen the drive belt idler pulley bolt.
2. Remove the drive belt idler pulley and bolt (1).

### Power Steering Pump Removal Procedure

1. Remove the power steering pump bolt. The bolt is located perpendicular to the crankshaft centerline and behind the power steering pulley.
2. Remove the power steering pump.

### Air Conditioning Compressor Removal Procedure

1. Remove the air conditioning compressor rear mounting bracket nut.
2. Remove the air conditioning compressor front mounting bolts.
3. Remove the air conditioning compressor by sliding off the rear mounting bracket stud.
4. Remove the air conditioning compressor stud.
5. Remove the air conditioning compressor rear mounting bracket bolts.
6. Remove the air conditioning compressor rear mounting bracket.

### Generator Removal Procedure

1. Remove the generator rear mounting bracket bolts from the engine block.
2. Remove the generator mounting bolts located at the front of the generator.
3. Remove the generator.
4. Remove the generator rear mounting bracket bolts from the generator.
5. Remove the generator rear mounting bracket.
6. Remove the generator front mounting bracket bolts from the block.
7. Remove the generator front mounting bracket.

### Drive Belt Tensioner Removal Procedure

1. Remove the drive belt tensioner bolt.
2. Remove the drive belt tensioner.