Battery Protection During Vehicle Storage. Cadillac Concours 1997

For 1990-2009 cars

In order to prevent parasitic load, disconnect the following components.

1. The negative battery cable
2. The radio fuse

Recharge the battery every 20-45 days until the hydrometer green dot is visible if the negative cable cannot be disconnected. Refer to Battery Charging .

Reset the following components once the vehicle is returned to service:

• | The radio presets

• | The HVAC controls (if automatic)

• | The driver information center (if equipped)

• | The clock