INTERMITTENT ITCH NOISE BETWEEN THE I/P TOP COVER. Cadillac Concours 1994

For 1990-2009 cars

# INTERMITTENT ITCH NOISE BETWEEN THE I/P TOP COVER

#### SUBJECT: INTERMITTENT ITCH NOISE BETWEEN THE I/P TOP COVER AND THE I/P WOOD TRIM (INSTALL FOAM TAPE)

#### MODELS: 1994 CADILLAC CONCOURS

#### CONDITION:

SOME OWNERS MAY COMMENT ON AN INTERMITTENT ITCH NOISE BETWEEN THE I/P TOP COVER AND THE I/P WOOD TRIM.

#### CAUSE:

CONTACT BETWEEN THE I/P TOP COVER AND THE I/P WOOD TRIM MAY CREATE THIS CONDITION.

#### CONDITION:

TO REPAIR THIS CONDITION, USE THE FOLLOWING PROCEDURE:

1. REMOVE THE UPPER I/P TRIM PAD AS PER SECTION 8C OF THE SERVICE MANUAL.

2. INSTALL "CLOSED CELL" FOAM TAPE ACROSS THE ENTIRE TOP EDGE OF I/P TRIM PANEL (SEE ILLUSTRATION).

3. INSTALL UPPER I/P TRIM PAD.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: C2362 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.