Transmission Slips in Reverse. Cadillac Concours 1996

For 1990-2009 cars

Checks | Causes
--- | ---
Fluid Level | Too high or too low
Line Pressure | Too low
Primary Pump | Gears worn or broken

Reverse Accumulator Seal and Housing

• | Seal cut

• | Oversize chamfer in bore

Reverse Band | Damaged, burned, slipping
Reverse Band Anchor Pins | Loose, missing
Reverse Clutch Plates | Damaged or burned
Reverse Clutch Seals | Cut, damaged or leaking
Reverse Servo Pin | Binding, too short
Reverse Servo Piston | Damaged or cracked
Reverse Servo Seals | Cut, damaged or leaking
Scavenge Pipe | Debris in pipe
Scavenge Pipe Seal | Cut or damaged
Scavenge Pump | Gears worn or broken