Forward and Coast Clutch Installation. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

J 39053 Forward and Coast Clutch Assembly Installer

Caution: The forward and coast clutch assembly weighs approximately 50 lbs. Personal injury may result if you drop the assembly.

1. Install the J 39053 into the forward and coast clutch and support assembly (636-834).
2. Using a chain hoist or suitable lifting equipment, install the forward and coast clutch and support assembly (636-834) into the barrel of the case. The two bolt holes and feed holes must line up with the holes in the bottom of the case.