Evaporative Emission Canister Purge Solenoid. Cadillac Concours 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the intake manifold top cover.
2. Remove the EVAP canister purge solenoid connector (1).
3. Remove the canister purge solenoid vaccum lines.
4. Remove the canister purge (2) solenoid valve bolt.
5. Remove the canister purge solenoid from the bracket.

### Installation Procedure

1. Install the canister purge solenoid to the bracket.
2. Install the canister purge solenoid (2) valve bolt.

Tighten
Tighten the bolt to 12 N·m (106 in lb).

Refer to the

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General information.
3. Install the canister purge solenoid vaccum lines.
4. Install the EVAP canister purge solenoid connector (1).
5. Install the bolt.

Tighten
Tighten the bolt to 10 N·m (7 lb in).

Refer to the

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
6. Install the intake manifold top cover.

Tighten
Tighten the bolt to 2 N·m (18 lb in).

Refer to the

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.