Engine Flywheel Installation. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

• | J 36660-A Torque Angle Meter

• | J 44214 Flywheel Holder

1. Apply sealant, GM P/N 12346004, (Canadian P/N 10953480), or equivalent, to the engine flywheel retaining bolts.
2. Place the engine flywheel in position on the crankshaft.
3. Slip one bolt into the engine flywheel washer.
4. Install the washer and bolt in a location at the top of its rotation allowing the engine flywheel to hang in position.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the remaining engine flywheel bolts.

5.1. | Install the J 44214 to the engine block.

5.2. | First Pass

Tighten
Tighten the engine flywheel retaining bolts to 15 N·m (11 lb ft).

5.3. | Final Pass

Tighten
Tighten the engine flywheel retaining bolts an additional 50 degrees using the J 36660-A .