DTC P0713 Transmission Fluid Temperature (TFT) Sensor Circuit High Input. Cadillac Concours 1997

For 1990-2009 cars
Automatic Transmission Components
TFP Val. Position Sw., TFT Sensor, and A/T ISS Sensor
Handling ESD Sensitive Parts Notice
OBD II Symbol Description Notice

### Circuit Description

The Automatic Transmission Fluid Temperature (TFT) sensor is a negative coefficient thermistor whose resistance value changes based on temperature. The Powertrain Control Module (PCM) provides a 5 volt reference to the sensor on circuit 1227. A low fluid temperature or open circuits 1227 or 452 result in high signal voltage. The TFT operating range is -40 to +151°C (-40 to +305°F).

If the PCM detects a continuous open or a short to power on the TFT sensor circuit, then DTC P0713 sets. DTC P0713 is a Type D DTC.

### Conditions for Setting the DTC

• | The engine is running.

• | The vehicle speed is more than 16 km/h (10 mph) for 5 minutes.

• | The engine coolant temperature is greater than -25°C (-13°F).

• | The PCM detects a reading of -40°C (-40°F) or less (5.04 volts or greater) for 6 seconds.

### Action Taken When the DTC Sets

• | The PCM does not illuminate the Malfunction Indicator Lamp (MIL).

• | If any engine coolant temperature sensor codes set, the PCM substitutes a transmission fluid temperature default value of 132°C (269°F).

• | If the engine coolant temperature is greater than 115°C (239°F), the PCM substitutes a transmission fluid temperature default value of 132°C (269°F). This enables Transmission Hot Mode. The transmission remains in Hot Mode until the engine coolant temperature drops below 110°C (230°F).

• | If the engine run time is less than 3 minutes, the PCM substitutes the intake air temperature for the transmission fluid temperature value at ignition ON.

• | If the engine coolant temperature is 45-115°C (113-239°F), the transmission fluid default temperature equals ECT-10°C when the intake air temperature is less than 27°C (81°F) at ignition ON. If the intake air temperature is greater than 27°C (81°F) at ignition ON, the transmission fluid default temperature equals ECT+10°C.

• | If engine run time is greater than 3 minutes and the engine coolant temperature is less than 45°C (113°F), the PCM substitutes a transmission fluid temperature default value of 12°C (54°F).

• | DTC P0713 is stored in the PCM history.

### Conditions for Clearing the DTC

• | A scan tool can clear the DTC from the PCM history. The PCM clears the DTC from the PCM history if the vehicle completes 40 warm-up cycles without a failure reported.

• | The PCM cancels the DTC default actions when the fault no longer exists and the ignition is OFF long enough in order to power down the PCM.

### Diagnostic Aids

• | Inspect the wiring for poor electrical connections at the PCM. Inspect the wiring for poor electrical connections at the transmission 20-way connector. Inspect the wiring for poor electrical connections at the Automatic Transmission Fluid Temperature sensor connector. Look for the following problems:

- | A bent terminal

- | A backed out terminal

- | A damaged terminal

- | Poor terminal tension

- | A chafed wire

- | A broken wire inside the insulation

- | Moisture intrusion

• | When diagnosing for an intermittent open, massage the wiring harness while watching the test equipment for a change.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. If the display does not indicate an Automatic Transmission Fluid Temperature Sensor voltage greater than 4.98 volts, inspect the connectors and the terminal for intermittent problems.

2. Important: After 7 seconds, the scan tool will display a default temperature.

   This step isolates the Automatic Transmission Wiring Harness by using a fused jumper from terminal M to the transmission case. Inspect Engine Wiring Harness circuit 1227 and circuit 452 for an open.

#### DTC P0713 Transmission Fluid Temperature Sensor Circuit High Input

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to A Powertrain On Board Diagnostic (OBD) System Check
2 | Has the transmission fluid checking procedure been performed? | -- | Go Step 3 | Go to Transmission Fluid Check

3

1. Install the Scan Tool ®.
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Failure Records for reference. Using the Clear Info function will erase the stored Failure Records from the PCM.

3. Record the DTC Failure Records, then clear the DTC.
4. Select TFT Sensor volts on the scan tool.

Does the scan tool display an Automatic Transmission Fluid Temperature voltage equal to or greater than the specified value?

4.98V

Go to Step 4

Go to Diagnostic Aids

4

1. Turn the ignition OFF.
2. Disconnect the transmission 20-way connector.
3. Install the J 39775 Jumper Harness to the engine side of the 20-way connector.
4. Using the J 35616-A Connector Test Adapter Kit, install a fused jumper wire from terminal M to the transmission case.
5. Turn the ignition ON, and keep the engine OFF.

Does the scan tool display an Automatic Transmission Fluid Temperature voltage equal to or greater than the specified value?

4.98V

Go to Step 5

Go to Step 7

5 | Inspect circuit 1227 of the Engine Wiring Harness for an open. Refer to Electrical Diagnosis, Section 8. Did you find and correct the condition? | -- | Go to Step 11 | Go to Step 6
6 | Inspect circuit 452 of the Engine Wiring Harness for an open. Refer to Electrical Diagnosis, Section 8. Did you find and correct the condition? | -- | Go to Step 11 | Go to Step 10

7

1. Inspect circuit 1227 of the Automatic Transmission Wiring Harness for an open.
2. Inspect circuit 452 for an open.

Refer to Electrical Diagnosis, Section 8.

Did you find the condition?

--

Go to Step 8

Go to Step 9

8 | Replace the Automatic Transmission Wiring Harness. Refer to Automatic Transmission Wiring Harness Replacement, in On-Vehicle Service. Is the replacement complete? | -- | Go to Step 11 | --
9 | Replace the Automatic Transmission Fluid Temperature sensor. Refer to Automatic Transmission Fluid Temperature Sensor Replacement, in On-Vehicle Service. Is the replacement complete? | -- | Go to Step 11 | --
10 | Replace the PCM. Refer to PCM Replacement/Programming Section 6. Is the replacement complete? | -- | Go to Step 11 | --

11

In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle under the following conditions:

• | Road test the vehicle.

• | The engine coolant temperature must be greater than -25°C (-13°F).

• | The vehicle speed must be greater than 16 km/h (10 mph) for more than 5 minutes.

4. Select Specific DTC. Enter DTC P0713.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1