Torque Converter and Oil Pump Drive Shaft Install. Cadillac Concours 1997

For 1990-2009 cars

1. Inspect the torque converter (1) lugs for damage and inspect the oil pump driven shaft for damage. Replace the turbine shaft seal (412).
2. Install the following parts:

• | The oil pump driven shaft (2) into the turbine shaft

• | The new turbine shaft O-ring seal (412)

• | The torque converter (1)

3. Remove the transmission from the base and then remove the holding fixture from the transmission.