Oil Filter and Side Cover Install. Cadillac Concours 1996

For 1990-2009 cars

1. Install the new filter seal (209) and the new oil filter (236).
2. Install the gasket (30) into the side cover (29).
3. Install the side cover onto the case cover.
4. Install the side cover bolts (28, 32).
5. Apply GM sealing adhesive 12346004 before installing the bolt (32).

Tighten
Tighten bolt (28) to 50-55 N·m (37-40 lb ft). Tighten bolt (32) to 20-27 N·m (15-20 lb ft).