Axle Seals Replacement. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

• | J 39051-1 Right Seal Driver

• | J 39051-2 Left Seal Driver

1. Using a screw driver remove the right and left axle seals (37, 125) by prying them out.
2. Using the J 39051-1 and the J 39051-2 , install the new axle seals (37, 125). Use the output shaft (57) to pilot the seals and the tool into the case. Ensure that the snap rings are installed on the output shaft.