STEERING COLUMN SHIFT LEVER BECOMES LOOSE. Cadillac Concours 1995

For 1990-2009 cars

# STEERING COLUMN SHIFT LEVER BECOMES LOOSE

#### SUBJECT: STEERING COLUMN SHIFT LEVER BECOMES LOOSE (APPLY LOCTITE(R) TO SPLINED SURFACE OF SHIFT LEVER PIN)

#### MODELS: 1995 CADILLAC CONCOURS, DEVILLE, ELDORADO, SEVILLE

#### CONDITION:

SOME OWNERS OF THE ABOVE LISTED VEHICLES MAY COMMENT ABOUT A CONDITION WHEREBY THE STEERING COLUMN SHIFT LEVER BECOMES LOOSE.

#### CORRECTION:

FOLLOWING THE SERVICE MANUAL PROCEDURE IN SECTION 3F, REMOVE SHIFT LEVER PIVOT PIN. BEFORE REINSTALLING SHIFT LEVER PIN, APPLY LOCTITE(R), OR EQUIVALENT, TO THE SPLINED SURFACE TO SECURE IN PLACE. REFER TO FIGURE 1, ITEM 1, FOR SHIFT LEVER PIN LOCATION.

#### IMPORTANT: APPLY LOCTITE(R), OR EQUIVALENT, ONLY TO THE SPLINED SURFACE OF SHIFT LEVER PIN.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: K5120 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 01 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.