SMU-SEC.8A-100/101/102 REV. CHART #2 (PARK LAMPS. Cadillac Concours 1997

For 1990-2009 cars

# SMU-SEC.8A-100/101/102 REV. CHART #2 (PARK LAMPS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTIONS 8A-100/101/102 - REVISED CHART #2 (PARK LAMPS AND HEADLAMPS INOPERATIVE)

#### MODELS: 1996-98 CADILLAC CONCOURS, DEVILLE, ELDORADO 1996-97 CADILLAC SEVILLE

THIS BULLETIN IS BEING ISSUED TO REVISE CHART #2 (PARK LAMPS AND HEADLAMPS INOPERATIVE) ON PAGE 8A-100-16 (1997-98 SERVICE MANUALS) AND PAGES 8A-101-14 AND 8A-102-9 (1996 SERVICE MANUAL).

THE BODY CONTROL MODULE (PZM) CONNECTOR C1 SHOULD NOT BE DISCONNECTED WHEN CHECKING FOR BATTERY VOLTAGE.

FIGURES: 00 ATTACHMENTS: 01

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.