SMU - Revised Fastener Tightening Specification for Cylinder Head Replacement. Cadillac Concours 1996

For 1990-2009 cars

# SMU - Revised Fastener Tightening Specification for Cylinder Head Replacement

Subject: | Revised Fastener Tightening Specification for Cylinder Head Replacement

Models: | 1996 Cadillac Concours

| 1996-97 Cadillac DeVille, Eldorado, Seville

| with 4.6L Engine (VINs Y, 9 -- RPOs LD8, L37)

This bulletin is being issued to revise a fastener tightening specification in the Cylinder Head Replacement procedure in the Engine Mechanical - 4.0L, 4.6L sub-section of the Service Manual. Please replace the current information in the Service Manual with the following information.

The following information has been updated within SI2000. If you are using a paper version of this Service Manual, please make a reference to this bulletin on the affected page.

When installing the three M6 bolts, tighten to 12 N·m (106 lb in).