Crankshaft Balancer Installation. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

• | J 41998-B Crankshaft Balancer Installer

• | J 36660-A Torque Angle Meter

• | J 44214 Flywheel Holder

1. Position the crankshaft balancer on the nose of the crankshaft.
2. Press the crankshaft balancer in place using the J 41998-B .
3. Clean the crankshaft balancer bolt threads.
4. Apply engine oil to the crankshaft balancer bolt threads.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the crankshaft balancer bolt.

5.1. | First Pass

Tighten
Tighten the crankshaft balancer bolt to 50 N·m (37 lb ft).

5.2. | Final Pass

Tighten
Tighten the crankshaft balancer bolt an additional 120 degrees using the J 36660-A .

6. Remove the J 44214 from the engine block.