Oil Pan Removal. Cadillac Concours 1996

For 1990-2009 cars

1. Rotate the engine so that the oil pan is facing up.
2. Remove the oil pan bolts.
3. Remove the oil pan from the lower crankcase oil distribution manifold plate.
4. Remove the oil pump pickup tube retaining nut (2) from the main bearing stud.
5. Remove the retaining bolt (4) from the oil manifold plate.
6. Remove the oil pump pickup tube (1).
7. Remove the oil pump tube O-ring (3).
8. Remove and discard the oil pan gasket.
9. Remove the oil level sensor (1).