INFO. ON ON-VEHICLE SERVICE OF THE UNIVERSAL GARAGE. Cadillac Concours 1995

For 1990-2009 cars

# INFO. ON ON-VEHICLE SERVICE OF THE UNIVERSAL GARAGE

#### SUBJECT: INFORMATION ON ON-VEHICLE SERVICE OF THE UNIVERSAL GARAGE DOOR OPENER (UGDO) TRANSMITTER

#### MODELS: 1995-96 CADILLAC CONCOURS, DEVILLE, ELDORADO, SEVILLE

GM OF CANADA AND NAES DEALERS ARE NOT AUTHORIZED TO UTILIZE THIS SERVICE BULLETIN.

INCORRECT REMOVAL PROCEDURES ARE CAUSING DAMAGE TO THE UNIVERSAL GARAGE DOOR OPENER (UGDO) TRANSMITTERS. USE OF THE 1994 MODEL YEAR PROCEDURE FOR REMOVAL WILL DAMAGE THE UGDO. DUE TO A DESIGN CHANGE TO REDUCE THEFT OF THE UGDO TRANSMITTER, THE ON-VEHICLE SERVICE PROCEDURE HAS CHANGED FOR 1995-96.

- ON-VEHICLE SERVICE IS LOCATED IN SECTION 9K-23 OF THE 1995 SERVICE MANUAL AND IN SECTION 9P OF THE 1996 SERVICE MANUAL.

ON-VEHICLE SERVICE: ELDORADO/SEVILLE

UGDO WITHOUT SUNROOF: ====================

REMOVE -

1. REMOVE TRIM PANEL.

2. TWO SCREWS.

3. SLIDE FORWARD AND DOWN FROM HEADLINER.

4. ELECTRICAL CONNECTOR.

5. DEPRESS TAB ON LOWER FRONT OF GARAGE DOOR OPENER FROM INSIDE OF HOUSING.

6. SLIDE GARAGE DOOR OPENER OUT THE ACCESS DOOR OF HOUSING.

INSTALL -

1. SLIDE GARAGE DOOR OPENER INTO ROOF CONSOLE THROUGH ACCESS DOOR.

- MAKE SURE THAT THE TAB SNAPS INTO PLACE.

2. POSITION OVERHEAD CONSOLE, SLIDE REARWARD AND UP.

3. TWO SCREWS.

4. TRIM PANEL TO OVERHEAD CONSOLE.

UGDO WITH SUNROOF: =================

REMOVE -

1. USING FLAT BLADED TOOL, POP TRIM PLATE FROM COVER, REFER TO FIGURE 1, ITEM 1 (PRY FROM FRONT SECTION OF TRIM PANEL; REAR SECTION HAS TABS, FRONT HAS FLEXIBLE RETAINERS).

2. ONE SCREW, REFER TO FIGURE 1, ITEM 2.

3. SLIDE FORWARD AND DOWN FROM HEADLINER.

4. ELECTRICAL CONNECTION.

5. DEPRESS TAB ON LOWER FRONT OF GARAGE DOOR OPENER FROM INSIDE OF HOUSING.

6. SLIDE GARAGE DOOR OPENER OUT THE ACCESS DOOR OF HOUSING.

INSTALL -

1. SLIDE GARAGE DOOR OPENER INTO ACCESS DOOR OF CONSOLE.

- MAKE SURE THAT THE TAB SNAPS INTO PLACE; AN AUDIBLE CLICK WILL BE HEARD.

2. POSITION OVERHEAD CONSOLE, SLIDE REARWARD AND UP.

3. SCREW.

4. TRIM PLATE.

ON-VEHICLE SERVICE: CONCOURS/DEVILLE

UGDO WITH OR WITHOUT SUNROOF: ============================

#### REMOVE:

1. RELEASE THE TABS AND REMOVE ROOF CONSOLE TRIM PLATE, REFER TO FIGURE 2, ITEM 2.

2. RELEASE TABS RETAINING SUNROOF SWITCH/ROOF SUPPORT.

3. MAP LAMP SWITCH CONNECTORS FROM CONSOLE.

4. ELECTRICAL CONNECTOR FROM GARAGE DOOR OPENER.

5. ROOF CONSOLE, REFER TO FIGURE 2, ITEM 1.

6. DEPRESS TAB ON LOWER FRONT OF GARAGE DOOR OPENER FROM INSIDE OF HOUSING.

7. SLIDE GARAGE DOOR OPENER OUT THE ACCESS DOOR OF HOUSING.

#### INSTALL:

1. SLIDE GARAGE DOOR OPENER INTO CONSOLE.

- MAKE SURE THAT THE TAB SNAPS INTO PLACE; AN AUDIBLE CLICK WILL BE HEARD.

2. WIRE LEADS (WITH BULB RETAINER) TO MAP LAMPS.

3. ELECTRICAL CONNECTOR TO GARAGE DOOR OPENER.

4. SUNROOF SWITCH/ROOF SUPPORT TO CONSOLE AND RETAIN WITH TABS.

5. CONSOLE TRIM PLATE.

FOR UGDO PROGRAMMING, REFER TO PROCEDURE IN SECTION 9P OF THE 1996 SERVICE MANUAL.

FIGURES: 2 ATTACHMENTS: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.