Case Cover/Turbine Shaft Seal Replacement. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

• | J 7079-2 Universal Driver Handle-Non Threaded

• | J 8092 Driver Handle

• | J 39062 Turbine Shaft Seal Tool

• | J 39648 Drive Sprocket Seal Installer

1. Using J 7079-2 (1) and the remover side of the J 39062 (2), remove the case cover to turbine shaft seal (35).
2. Using a small screwdriver, remove the case cover to drive sprocket seal (34) by tapping the seal out through the slots in the case cover.
3. Using J 7079-2 (1) the installer side of the J 39062 (2), install the case cover to turbine shaft seal (35).
4. Using J 8092 (1) and J 39648 (2), install the case cover to drive sprocket seal (34).