Transmission Fluid Level Indicator Replacement. Cadillac Concours 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the fluid-level indicator at the transmission. Rotate the indicator counterclockwise to unlock, then pull the indicator straight out of the transmission.
2. Inspect the O-ring seal on the indicator for nicks. Replace the seal, if damaged.

### Installation Procedure

1. Install the fluid-level indicator at the transmission.
2. Push the indicator straight into the transmission. Rotate clockwise in order to lock.