Parking Pawl and Pivot Pin Install. Cadillac Concours 1996

For 1990-2009 cars

1. Place the parking pawl (22) into the case slot.
2. Install the parking pawl pivot pin (23) into the case.
3. Install the parking pawl spring over the parking pawl. The hook end of the spring locates on the case, and the square end goes on top of the parking pawl.
4. Tap the parking pawl pivot pin (23) in place while pressing down on the pawl and spring assembly (25).
5. Verify the correct function of the parking pawl by moving the manual shaft and detent lever through the different ranges. Then return the manual shaft to the Park position.