Control Valve Upper Body Assemble. Cadillac Concours 1996

For 1990-2009 cars

1. Inspect all valve body passages for debris, and then inspect the gasket for damage.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the automatic transmission fluid temperature sensor (350).

Tighten
Tighten the automatic transmission fluid temperature sensor to 3.4 N·m (30 lb in).

3. Install the following parts:

• | The 1-2, 3-4 accumulator valves (301, 302)

• | The bushing (303)

• | The coiled spring pin (304)

4. Install the following parts:

• | The 2-3 accumulator valve (306)

• | The bore plug (307)

• | The retainer clip (308)

5. Install the following parts:

• | The actuator feed limit valve (309)

• | The actuator feed limit valve spring (310)

• | The spring retaining plate (311)

6. Install the following parts:

• | The converter feed limit valve (312)

• | The converter feed limit valve spring (313)

• | The bore plug (307)

• | The retaining clip (308)

7. Install the following parts:

• | The torque converter clutch enable valve (322)

• | The torque converter clutch enable valve spring (323)

• | The bore plug (307)

• | The retainer clip (308)

8. Install the following parts:

• | The converter regulator valve (318)

• | The converter regulator valve spring (319)

• | The bore plug (307)

• | The retainer clip (308)

9. Install the following parts:

• | The converter clutch control spring (316)

• | The converter clutch control valve (317)

• | The coiled spring pin (304)

• | The torque converter clutch solenoid valve (336)

• | The spring retainer clip from the torque converter clutch solenoid valve (337)

10. Install the following parts:

• | The pressure control solenoid filter and seal (338)

• | The pressure control solenoid valve (339)

• | The pressure control solenoid clamp (340)

11. Install the clamp bolt (15).

Tighten
Tighten the bolt to 11-13 N·m (8.0-9.5 lb ft).

12. Install the following parts:

• | The 2-3 accumulator pin (348)

• | The snap ring (349)

• | The 2-3 accumulator piston spring (347)

• | The accumulator piston and seal (345, 346)

• | The 2-3 piston cushion spring (351)