EXCESSIVE TWIST OR FLEXING OF REAR COMPARTMENT LID. Cadillac Concours 1994

For 1990-2009 cars

# EXCESSIVE TWIST OR FLEXING OF REAR COMPARTMENT LID

REVISION: 01/26/95

THIS BULLETIN IS BEING REVISED TO INCLUDE ADDITIONAL WARRANTY INFORMATION. *********************************************************************

#### SUBJECT: EXCESSIVE TWIST OR FLEXING OF THE REAR COMPARTMENT LID WHEN CLOSING FROM SIDE OF VEHICLE (REPLACE LID, TORQUE RODS AND LOCK CYLINDER)

#### MODELS: 1994 CADILLAC CONCOURS AND DEVILLE (BUILT PRIOR TO VIN RU291053)

#### CONDITION:

SOME OWNERS MAY COMMENT ON EXCESSIVE TWISTING OR FLEXING OF THE REAR COMPARTMENT LID WHEN CLOSING THE LID FROM THE SIDE OF THE VEHICLE.

#### CAUSE:

THE GAUGE OF THE METAL IN THE LID ASSEMBLY ALLOWS FOR EXCESSIVE FLEXING.

#### CORRECTION:

THE REAR COMPARTMENT LID HAS A NEW DESIGN. THE ABOVE CONDITION HAS BEEN CORRECTED BY INCREASING THE THICKNESS OF THE LID INNER PANEL. IF LID REPLACEMENT IS REQUIRED ON VEHICLES BUILT PRIOR TO THE AFFECTED VIN BREAKPOINT (SEE ABOVE), THE VEHICLE MUST BE RETROFITTED WITH A NEW LID, TORQUE RODS AND LOCK CYLINDER COVER. VEHICLES BUILT AFTER THE AFFECTED VIN BREAKPOINT DO NOT REQUIRE REPLACEMENT OF THESE COMPONENTS UNLESS THEY HAVE BEEN DAMAGED.

1. REPLACE REAR COMPARTMENT LID, P/N 25634540. REFER TO SECTION 10-8 OF THE SERVICE MANUAL FOR REPLACEMENT PROCEDURE.

2. REPLACE TORQUE RODS, P/N 3549126 AND 3549127. REFER TO SECTION 10-8 OF THE SERVICE MANUAL FOR REPLACEMENT PROCEDURE.

3. REPLACE LOCK CYLINDER COVER, P/N 25636490 (DEVILLE) OR P/N 25636491 (CONCOURS). REFER TO SECTION 10-1 OF THE SERVICE MANUAL UNDER ADHESIVE MOLDING AND NAMEPLATE REPLACEMENT.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: T2454 (TO REPLACE REAR COMPARTMENT LID, TORQUE RODS, LOCK CYLINDER) LABOR TIME: 1.3 HR.

ADD: FOR PAINTING OF REAR COMPARTMENT LID, ADD PUBLISHED REFINISH TIMES AND PAINT MIX TIME FROM APPLICABLE GM LABOR TIME GUIDE (A2730) TO LABOR HOURS IN T2454; SHOW APPLICABLE PAINT MATERIAL IN NET ITEM FIELD.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.