HORN HARD TO OPERATE WHEN COLD (REPLACE HORN PAD. Cadillac Concours 1997

For 1990-2009 cars

# HORN HARD TO OPERATE WHEN COLD (REPLACE HORN PAD

#### SUBJECT: HORN HARD TO OPERATE WHEN COLD (REPLACE HORN PAD/AIRBAG MODULE)

#### MODELS: 1996-97 CADILLAC CONCOURS, DEVILLE, D'ELEGANCE, ELDORADO, SEVILLE

BUILT PRIOR TO VIN BREAKPOINTS:

CONCOURS VU227956 DEVILLE/D'ELEGANCE/SEVILLE VU810505 ELDORADO VU606045

#### CONDITION:

SOME OWNERS MAY COMMENT ON EXCESSIVE FORCE REQUIRED TO OPERATE THE HORN WHEN COLD.

#### CORRECTION:

TO CORRECT THIS CONDITION, REPLACE THE HORN PAD (INFLATABLE RESTRAINT STEERING WHEEL MODULE) WITH ONE OF THE FOLLOWING PART NUMBERS LISTED BELOW.

#### PARTS INFORMATION:

YEAR COLOR P/N ==== ===== ===

96 BLACK 16822087 96 BORDEAUX RED 16822088 96 DARK MONTANA BLUE 16822089 96 MED BEECHWOOD 16822090 96 SHALE 16822091 96 CAPPUCCINO CREAM 16822092 96 CRYSTAL GREEN 16822093

97 BLACK 16822094 97 MEDICI RED 16822095 97 DARK MONTANA BLUE 16822096 97 MED BEECHWOOD 16822097 97 SHALE 16822098 97 CAPPUCCINO CREAM 16822099 97 CRYSTAL GREEN 16822100

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: C8835 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.