Fastener Tightening Specifications. Cadillac Concours 1997

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Conditioning Compressor Bracket to Lower Crankcase Lock Nut | 30 N·m | 22 lb ft
Air Conditioning Compressor Bracket to Lower Crankcase Stud | 25 N·m | 18 lb ft
Air Conditioning Compressor to Block and Bracket | 50 N·m | 37 lb ft
Air Conditioning Compressor Mounting Bracket to Compressor | 25 N·m | 18 lb ft
Brace--Left Bank (Long) | 75 N·m | 55 lb ft
Brace--Left Bank (Short) | 50 N·m | 37 lb ft
Braces--Right Bank | 50 N·m | 37 lb ft
Camshaft Bearing Cap | 12 N·m | 106 lb in
Camshaft Chain Guide Access Plug | 4.5 N·m | 39 lb in
Camshaft Cover | 10 N·m | 89 lb in
Camshaft Drive Chain Guide Bolts | 25 N·m | 18 lb ft
Camshaft Drive Chain Tensioner to Block | 25 N·m | 18 lb ft
Camshaft Seal Retainer to Cam Cover (Left Hand Head) | 3 N·m | 27 lb in
Camshaft Sprocket | 120 N·m | 89 lb ft
Catalytic Converter to Exhaust Manifold Rear Pipe | 50 N·m | 37 lb ft
Connecting Rod Bolt

- First Pass

30 N·m

22 lb ft

- Second Pass

Back off to zero

- Third Pass

25 N·m

18 lb ft

- Final Pass

+110 degrees

Coolant Temperature Sensor | 20 N·m | 15 lb ft
Crankshaft Balancer Bolt

- First Pass

50 N·m

37 lb ft

- Final Pass

+120 degrees

Crankshaft Position Sensor | 10 N·m | 89 lb in
Cruise Control Bracket to Throttle Body Bracket | 12 N·m | 106 lb in
Cylinder Block Coolant Heater - Right & Left | 10 N·m | 89 lb in
Cylinder Head Bolt (M11)

- First Pass

40 N·m

30 lb ft

- Second Pass

+70 degrees

- Third Pass

+60 degrees

- Final Pass

+60 degrees (190 degrees Total)

Cylinder Head Bolt (M6) | 12 N·m | 106 lb in
Cylinder Head Plug | 80 N·m | 59 lb ft
Cylinder Head Plug (Oil Gallery) | 12 N·m | 106 lb in
Cylinder Head Plug (Soc Hex) | 5.5 N·m | 49 lb in
Drive Belt Idler Pulley | 50 N·m | 37 lb ft
Drive Belt Tensioner | 50 N·m | 37 lb ft
EGR Pipe (to Intake Manifold) | 25 N·m | 18 lb ft
EGR Tube (to Water Crossover) | 25 N·m | 18 lb ft
EGR Tube to Intermediate Pipe Nut | 60 N·m | 44 lb ft
EGR Valve | 25 N·m | 18 lb ft
Engine Flywheel Bolt

- First Pass

15 N·m

11 lb ft

- Final Pass

+50 degrees

Exhaust Manifold Pipe to Cylinder Head | 25 N·m | 18 lb ft
Exhaust Manifold Pipe to EGR Tube | 60 N·m | 44 lb ft
Exhaust Manifold Pipe to Exhaust Manifold Rear Pipe | 25 N·m | 18 lb ft
Exhaust Manifold Pipe to Lower Crankcase | 25 N·m | 18 lb ft
Exhaust Manifold Rear Pipe to Right Manifold | 40 N·m | 30 lb ft
Exhaust Manifold to Cylinder Head Lock Nut | 25 N·m | 18 lb ft
Exhaust Manifold to Cylinder Head Bolt | 25 N·m | 18 lb ft
Flywheel Housing Cover Bolt | 9 N·m | 80 lb in
Front Cover Bolt | 10 N·m | 89 lb in
Generator and Air Conditioning Bracket to Block Bolt | 50 N·m | 37 lb ft
Generator Bracket to Block (Rear Bolt) | 47 N·m | 35 lb ft
Generator Bracket to Block (Rear Nut) | 38 N·m | 28 lb ft
Generator to Bracket (Front Lower Bolt) | 50 N·m | 37 lb ft
Generator to Bracket (Front Upper Bolt) | 50 N·m | 37 lb ft
Generator to Bracket (Rear Bolt) | 50 N·m | 37 lb ft
Ignition Module Bolt (to Cam Cover) | 12 N·m | 106 lb in
Intake Manifold Bolt | 10 N·m | 89 lb in
Intermediate Sprocket Retaining Bolt | 60 N·m | 44 lb ft
Intermediate Sprocket Shaft Bolt | 10 N·m | 89 lb in
Knock Sensor | 20 N·m | 15 lb ft
Lift Bracket--Front | 50 N·m | 37 lb ft
Lift Bracket--Right Rear | 50 N·m | 37 lb ft
Lower Crankcase to Block (M8 x 1.25) | 30 N·m | 22 lb ft
Lower Crankcase Bolt/Stud (In Sequence) (M10 x 1.5)

- First Pass

20 N·m

15 lb ft

- Final Pass

+65 degrees

Oil Cooler lines to Oil Cooler | 18 N·m | 13 lb ft
Oil Cooler Lines to Oil Filter Adapter | 18 N·m | 13 lb ft
Oil Filter Adapter | 16 N·m | 12 lb ft
Oil Filter Adapter Plug w/Oil Cooler | 20 N·m | 15 lb ft
Oil Filter Adapter Plug w/o Oil Cooler | 18 N·m | 13 lb ft
Oil Level Indicator Tube | 10 N·m | 89 lb in
Oil Level Sensor | 20 N·m | 15 lb ft
Oil Manifold Plate to Lower Crankcase | 10 N·m | 89 lb in
Oil Pan Bolt

- First Pass

8 N·m

71 lb in

- Final Pass

12 N·m

106 lb in

Oil Pan Brace | 50 N·m | 37 lb ft
Oil Pan Drain Plug | 20 N·m | 15 lb ft
Oil Pump Suction Pipe (Lock Nut) | 25 N·m | 18 lb ft
Oil Pump to Lower Crankcase

- First Pass

10 N·m

89 lb in

- Final Pass

+35 degrees

Oxygen Sensor | 40 N·m | 30 lb ft
Power Steering Pump (to Bracket) | 25 N·m | 18 lb ft
Power Steering Pump Bracket (to Block) | 50 N·m | 37 lb ft
Starter (to Block) | 30 N·m | 22 lb ft
Starter Motor (Lock Nut) | 10 N·m | 89 lb in
Thermostat Outlet to Water Pump Cover | 10 N·m | 89 lb in
Torque Converter to Flywheel Bolt | 47 N·m | 35 lb ft
Torque Strut Bracket to Cylinder Head | 50 N·m | 37 lb ft
Torque Strut Bracket to Cylinder Head (Stud) | 50 N·m | 37 lb ft
Torque Strut Bracket to Water Manifold | 25 N·m | 18 lb ft
Transaxle Bel Housing to Engine | 75 N·m | 55 lb ft
Water Crossover (to Block) | 25 N·m | 18 lb ft
Water Crossover (to Head) | 25 N·m | 18 lb ft
Water Crossover Plug | 25 N·m | 18 lb ft
Water Outlet Fitting | 50 N·m | 37 lb ft
Water Outlet to Cylinder Head | 25 N·m | 18 lb ft
Water Pump Assembly | 100 N·m | 74 lb ft
Water Pump Drive Belt Shield Retaining Bolt | 10 N·m | 89 lb in
Water Pump Drive Belt Shield Retaining Nut | 10 N·m | 89 lb in
Water Pump Drive Belt Tensioner to Water Crossover (Stud) | 10 N·m | 89 lb in
Water Pump Cover to Water Pump Housing | 10 N·m | 89 lb in