Fastener Tightening Specifications. Cadillac Concours 1997

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable to Generator Output Stud | 20 N·m | 15 lb ft
Battery Cables to Battery | 15 N·m | 11 lb ft
Battery Cables to Starter | 17 N·m | 13 lb ft
Battery Cable Nut at Solenoid | 8 N·m | 71 lb in
Battery Cable Retaining Clips | 6 N·m | 53 lb in
Battery Retainer Bolt | 8 N·m | 71 lb in
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Flywheel Inspection Cover Bolts | 15 N·m | 11 lb tf
Generator Mounting Bolt (Front Lower) | 47 N·m | 35 lb ft
enerator Mounting Bolt (Upper) | 47 N·m | 35 lb ft
Generator Mounting Bolt (Upper Rear) | 47 N·m | 35 lb ft
Generator Bracket Bolts | 47 N·m | 35 lb ft
Generator Output Cable | 20 N·m | 15 lb ft
Ignition Control Module Bolts | 12 N·m | 106 lb in
Knock Sensor | 19 N·m | 14 lb ft
Solenoid S Terminal Nut | 3 N·m | 26 lb in
Spark Plugs | 15 N·m | 11 lb ft
Starter Motor Mounting Bolts | 30 N·m | 22 lb ft